14.3. Encoding with the `libavcodec` codec family
Пред. | Глава 14. Encoding with MEncoder | След.

## 14.3. Encoding with the `libavcodec` codec family

`libavcodec` provides simple encoding to a lot of interesting video and audio formats. You can encode to the following codecs (more or less up to date):

### 14.3.1. `libavcodec`'s video codecs

Video codec name | Description
--- | ---
mjpeg | Motion JPEG
ljpeg | lossless JPEG
h261 | H.261
h263 | H.263
h263p | H.263+
mpeg4 | ISO standard MPEG-4 (DivX, XviD compatible)
msmpeg4 | pre-standard MPEG-4 variant by MS, v3 (AKA DivX3)
msmpeg4v2 | pre-standard MPEG-4 by MS, v2 (used in old ASF files)
wmv1 | Windows Media Video, version 1 (AKA WMV7)
wmv2 | Windows Media Video, version 2 (AKA WMV8)
rv10 | RealVideo 1.0
rv20 | RealVideo 2.0
mpeg1video | MPEG-1 video
mpeg2video | MPEG-2 video
huffyuv | lossless compression
asv1 | ASUS Video v1
asv2 | ASUS Video v2
ffv1 | FFmpeg's lossless video codec
svq1 | Sorenson video 1
flv | Sorenson H.263 used in Flash Video
dvvideo | Sony Digital Video
snow | FFmpeg's experimental wavelet-based codec

The first column contains the codec names that should be passed after the `vcodec` config, like: `-lavcopts vcodec=msmpeg4`

An example with MJPEG compression:

    mencoder dvd://2 -o title2.avi -ovc lavc -lavcopts vcodec=mjpeg -oac copy

### 14.3.2. `libavcodec`'s audio codecs

Audio codec name | Description
--- | ---
mp2 | MPEG Layer 2
ac3 | AC3, AKA Dolby Digital
adpcm_ima_wav | IMA adaptive PCM (4 bits per sample, 4:1 compression)
sonic | experimental lossy/lossless codec

The first column contains the codec names that should be passed after the `acodec` option, like: `-lavcopts acodec=ac3`

An example with AC3 compression:

    mencoder dvd://2 -o title2.avi -oac lavc -lavcopts acodec=ac3 -ovc copy

Contrary to `libavcodec`'s video codecs, its audio codecs do not make a wise usage of the bits they are given as they lack some minimal psychoacoustic model (if at all) which most other codec implementations feature. However, note that all these audio codecs are very fast and work out-of-the-box everywhere MEncoder has been compiled with `libavcodec` (which is the case most of time), and do not depend on external libraries.

### 14.3.3. Encoding options of libavcodec

Ideally, you would probably want to be able to just tell the encoder to switch into "high quality" mode and move on. That would probably be nice, but unfortunately hard to implement as different encoding options yield different quality results depending on the source material. That is because compression depends on the visual properties of the video in question. For example, anime and live action have very different properties and thus require different options to obtain optimum encoding. The good news is that some options should never be left out, like `mbd=2`, `trell`, and `v4mv`. See below for a detailed description of common encoding options.

Options to adjust:

- vmax_b_frames: 1 or 2 is good, depending on the movie. Note that if you need to have your encode be decodable by DivX5, you need to activate closed GOP support, using `libavcodec`'s `cgop` option, but you need to deactivate scene detection, which is not a good idea as it will hurt encode efficiency a bit.

- vb_strategy=1: helps in high-motion scenes. On some videos, vmax_b_frames may hurt quality, but vmax_b_frames=2 along with vb_strategy=1 helps.

- dia: motion search range. Bigger is better and slower. Negative values are a completely different scale. Good values are -1 for a fast encode, or 2-4 for slower.

- predia: motion search pre-pass. Not as important as dia. Good values are 1 (default) to 4. Requires preme=2 to really be useful.

- cmp, subcmp, precmp: Comparison function for motion estimation. Experiment with values of 0 (default), 2 (hadamard), 3 (dct), and 6 (rate distortion). 0 is fastest, and sufficient for precmp. For cmp and subcmp, 2 is good for anime, and 3 is good for live action. 6 may or may not be slightly better, but is slow.

- last_pred: Number of motion predictors to take from the previous frame. 1-3 or so help at little speed cost. Higher values are slow for no extra gain.

- cbp, mv0: Controls the selection of macroblocks. Small speed cost for small quality gain.

- qprd: adaptive quantization based on the macroblock's complexity. May help or hurt depending on the video and other options. This can cause artifacts unless you set vqmax to some reasonably small value (6 is good, maybe as low as 4); vqmin=1 should also help.

- qns: very slow, especially when combined with qprd. This option will make the encoder minimize noise due to compression artifacts instead of making the encoded video strictly match the source. Do not use this unless you have already tweaked everything else as far as it will go and the results still are not good enough.

- vqcomp: Tweak ratecontrol. What values are good depends on the movie. You can safely leave this alone if you want. Reducing vqcomp puts more bits on low-complexity scenes, increasing it puts them on high-complexity scenes (default: 0.5, range: 0-1. recommended range: 0.5-0.7).

- vlelim, vcelim: Sets the single coefficient elimination threshold for luminance and chroma planes. These are encoded separately in all MPEG-like algorithms. The idea behind these options is to use some good heuristics to determine when the change in a block is less than the threshold you specify, and in such a case, to just encode the block as "no change". This saves bits and perhaps speeds up encoding. vlelim=-4 and vcelim=9 seem to be good for live movies, but seem not to help with anime; when encoding animation, you should probably leave them unchanged.

- qpel: Quarter pixel motion estimation. MPEG-4 uses half pixel precision for its motion search by default, therefore this option comes with an overhead as more information will be stored in the encoded file. The compression gain/loss depends on the movie, but it is usually not very effective on anime. qpel always incurs a significant cost in CPU decode time (+25% in practice).

- psnr: does not affect the actual encoding, but writes a log file giving the type/size/quality of each frame, and prints a summary of PSNR (Peak Signal to Noise Ratio) at the end.

Options not recommended to play with:

- vme: The default is best.

- lumi_mask, dark_mask: Psychovisual adaptive quantization. You do not want to play with those options if you care about quality. Reasonable values may be effective in your case, but be warned this is very subjective.

- scplx_mask: Tries to prevent blocky artifacts, but postprocessing is better.

### 14.3.4. Encoding setting examples

The following settings are examples of different encoding option combinations that affect the speed vs quality tradeoff at the same target bitrate.

All the encoding settings were tested on a 720x448 @30000/1001 fps video sample, the target bitrate was 900kbps, and the machine was an AMD-64 3400+ at 2400 MHz in 64 bits mode. Each encoding setting features the measured encoding speed (in frames per second) and the PSNR loss (in dB) compared to the "very high quality" setting. Please understand that depending on your source, your machine type and development advancements, you may get very different results.

Description | Encoding options | speed (in fps) | Relative PSNR loss (in dB)
--- | --- | --- | ---
Very high quality | `vcodec=mpeg4:mbd=2:mv0:trell:v4mv:cbp:last_pred=3:predia=2:dia=2:vmax_b_frames=2:vb_strategy=1:precmp=2:cmp=2:subcmp=2:preme=2:qns=2` | 6fps | 0dB
High quality | `vcodec=mpeg4:mbd=2:trell:v4mv:last_pred=2:dia=-1:vmax_b_frames=2:vb_strategy=1:cmp=3:subcmp=3:precmp=0:vqcomp=0.6:turbo` | 15fps | -0.5dB
Fast | `vcodec=mpeg4:mbd=2:trell:v4mv:turbo` | 42fps | -0.74dB
Realtime | `vcodec=mpeg4:mbd=2:turbo` | 54fps | -1.21dB

### 14.3.5. Custom inter/intra matrices

With this feature of `libavcodec` you are able to set custom inter (I-frames/keyframes) and intra (P-frames/predicted frames) matrices. It is supported by many of the codecs: `mpeg1video` and `mpeg2video` are reported as working.

A typical usage of this feature is to set the matrices preferred by the KVCD specifications.

The KVCD "Notch" Quantization Matrix:

Intra:

     8  9 12 22 26 27 29 34
     9 10 14 26 27 29 34 37
    12 14 18 27 29 34 37 38
    22 26 27 31 36 37 38 40
    26 27 29 36 39 38 40 48
    27 29 34 37 38 40 48 58
    29 34 37 38 40 48 58 69
    34 37 38 40 48 58 69 79

Inter:

    16 18 20 22 24 26 28 30
    18 20 22 24 26 28 30 32
    20 22 24 26 28 30 32 34
    22 24 26 30 32 32 34 36
    24 26 28 32 34 34 36 38
    26 28 30 32 34 36 38 40
    28 30 32 34 36 38 42 42
    30 32 34 36 38 40 42 44

Usage:

    $ mencoder input.avi -o output.avi -oac copy -ovc lavc -lavcopts inter_matrix=...:intra_matrix=...

    $ mencoder input.avi -ovc lavc -lavcopts
    vcodec=mpeg2video:intra_matrix=8,9,12,22,26,27,29,34,9,10,14,26,27,29,34,37,
    12,14,18,27,29,34,37,38,22,26,27,31,36,37,38,40,26,27,29,36,39,38,40,48,27,
    29,34,37,38,40,48,58,29,34,37,38,40,48,58,69,34,37,38,40,48,58,69,79
    :inter_matrix=16,18,20,22,24,26,28,30,18,20,22,24,26,28,30,32,20,22,24,26,
    28,30,32,34,22,24,26,30,32,32,34,36,24,26,28,32,34,34,36,38,26,28,30,32,34,
    36,38,40,28,30,32,34,36,38,42,42,30,32,34,36,38,40,42,44 -oac copy -o svcd.mpg

### 14.3.6. Example

So, you have just bought your shiny new copy of Harry Potter and the Chamber of Secrets (widescreen edition, of course), and you want to rip this DVD so that you can add it to your Home Theatre PC. This is a region 1 DVD, so it is NTSC. The example below will still apply to PAL, except you will omit `-ofps 24000/1001` (because the output framerate is the same as the input framerate), and of course the crop dimensions will be different.

After running `mplayer dvd://1`, we follow the process detailed in the section How to deal with telecine and interlacing in NTSC DVDs and discover that it is 24000/1001 fps progressive video, which means that we need not use an inverse telecine filter, such as `pullup` or `filmdint`.

Next, we want to determine the appropriate crop rectangle, so we use the cropdetect filter:

    mplayer dvd://1 -vf cropdetect

Make sure you seek to a fully filled frame (such as a bright scene), and you will see in MPlayer's console output:

    crop area: X: 0..719  Y: 57..419  (-vf crop=720:362:0:58)

We then play the movie back with this filter to test its correctness:

    mplayer dvd://1 -vf crop=720:362:0:58

And we see that it looks perfectly fine. Next, we ensure the width and height are a multiple of 16. The width is fine, however the height is not. Since we did not fail 7th grade math, we know that the nearest multiple of 16 lower than 362 is 352.

We could just use `crop=720:352:0:58`, but it would be nice to take a little off the top and a little off the bottom so that we retain the center. We have shrunk the height by 10 pixels, but we do not want to increase the y-offset by 5-pixels since that is an odd number and will adversely affect quality. Instead, we will increase the y-offset by 4 pixels:

    mplayer dvd://1 -vf crop=720:352:0:62

Another reason to shave pixels from both the top and the bottom is that we ensure we have eliminated any half-black pixels if they exist. Note that if your video is telecined, make sure the `pullup` filter (or whichever inverse telecine filter you decide to use) appears in the filter chain before you crop. If it is interlaced, deinterlace before cropping. (If you choose to preserve the interlaced video, then make sure your vertical crop offset is a multiple of 4.)

If you are really concerned about losing those 10 pixels, you might prefer instead to scale the dimensions down to the nearest multiple of 16. The filter chain would look like:

    -vf crop=720:362:0:58,scale=720:352

Scaling the video down like this will mean that some small amount of detail is lost, though it probably will not be perceptible. Scaling up will result in lower quality (unless you increase the bitrate). Cropping discards those pixels altogether. It is a tradeoff that you will want to consider for each circumstance. For example, if the DVD video was made for television, you might want to avoid vertical scaling, since the line sampling corresponds to the way the content was originally recorded.

On inspection, we see that our movie has a fair bit of action and high amounts of detail, so we pick 2400Kbit for our bitrate.

We are now ready to do the two pass encode. Pass one:

    mencoder dvd://1 -ofps 24000/1001 -oac copy -vf pullup,softskip,crop=720:352:0:62,hqdn3d=2:1:2 -ovc lavc \
    -lavcopts vcodec=mpeg4:vbitrate=2400:v4mv:mbd=2:trell:cmp=3:subcmp=3:mbcmp=3:autoaspect:vpass=1 \
    -o Harry_Potter_2.avi

And pass two is the same, except that we specify `vpass=2`:

    mencoder dvd://1 -ofps 24000/1001 -oac copy -vf pullup,softskip,crop=720:352:0:62,hqdn3d=2:1:2 -ovc lavc \
    -lavcopts vcodec=mpeg4:vbitrate=2400:v4mv:mbd=2:trell:cmp=3:subcmp=3:mbcmp=3:autoaspect:vpass=2 \
    -o Harry_Potter_2.avi

The options `v4mv:mbd=2:trell` will greatly increase the quality at the expense of encoding time. There is little reason to leave these options out when the primary goal is quality. The options `cmp=3:subcmp=3:mbcmp=3` select a comparison function that yields higher quality than the defaults. You might try experimenting with this parameter (refer to the man page for the possible values) as different functions can have a large impact on quality depending on the source material. For example, if you find `libavcodec` produces too much blocky artifacting, you could try selecting the experimental NSSE as comparison function via `*cmp=10`.

For this movie, the resulting AVI will be 138 minutes long and nearly 3GB. And because you said that file size does not matter, this is a perfectly acceptable size. However, if you had wanted it smaller, you could try a lower bitrate. Increasing bitrates have diminishing returns, so while we might clearly see an improvement from 1800Kbit to 2000Kbit, it might not be so noticeable above 2000Kbit. Feel free to experiment until you are happy.

Because we passed the source video through a denoise filter, you may want to add some of it back during playback. This, along with the `spp` post-processing filter, drastically improves the perception of quality and helps eliminate blocky artifacts in the video. With MPlayer's `autoq` option, you can vary the amount of post-processing done by the spp filter depending on available CPU. Also, at this point, you may want to apply gamma and/or color correction to best suit your display. For example:

    mplayer Harry_Potter_2.avi -vf spp,noise=9ah:5ah,eq2=1.2 -autoq 3

Пред. | Уровень выше | След.
14.2. How to deal with telecine and interlacing within NTSC DVDs | Начало | 14.4. Encoding with the `XviD` codec